Swap servoPWM and ESGPIO1

Change the 3.5K resistor on 24V LED to 3K

Change the name of the LDO if it’s still out of stock

Tie CP2102 EP to GND

Change autoreset circuit capacitor to 1uF

FP of CAN 60ohm resistors

Add ICLR logo

Antenna line isn’t 50ohms because the H used was wrong, new W = 0.700665